# Funktionsreferenz

_viGTL

"Go To Local"-Modus:
Instrumente, die dieses Kommando akzeptieren, werden den "Remote Control mode" verlassen und in den "Local mode" wechseln.
Wenn das Instrument schon im "Local mode" ist, wird der Befehl einfach irgnoriert.
Ein instrument, das diese Funktion nicht unterstützt, wird normalerweise im "Remote Control mode" verbleiben.

#include <Visa.au3>
_viGTL($h_session)

Parameter

$h_session | Ein VISA descriptor (STRING) ODER ein VISA session handle (INTEGER). Für mehr Informationen, siehe die Bemerkungen zu _viExecCommand.

Bemerkungen

Wie für alle VISA Funktionen müssen die VISA Bibliotheken installiert sein (prüfe ob die visa32.dll in {WINDOWS}\system32 vorhanden ist) und eine GPIB Karte (wie z.B. National Instruments NI PCI-GPIB Karte oder die Agilent 82350B PCI High-Performance GPIB Karte) installiert sein.
* Eine detaillierte Beschreibung der bekanntesten VISA DESCRIPTORS ist in den Bemerkungen zu der Funktion "_viExecCommand" zu finden.

Siehe auch

_viExecCommand, _viGpibBusReset, _viFindGpib, _viOpen, _viClose

Beispiel

;- This assumes that you have instrument set to GPIB address 3
; If you have an instrument in a different address change "GPIB::3::0" to the
; corresponding descriptor. Do the same for the call to _viOpen
; It shows how to use the _viGTL function with a VISA descriptor and with a
; VISA device handler. We use _viExecCommand first to force the instrument to go
; into "Remote mode"
#include <Visa.au3>
Dim $h_session = 0
; Query the ID of the instrument in GPIB address 3
MsgBox(0,"Step 1","Simple GPIB query using a VISA Descriptor")
Dim $s_answer = _viExecCommand("GPIB::3::0","*IDN?",10)
MsgBox(0,"GPIB QUERY result",$s_answer) ; Show the answer
MsgBox(0,"Step 2","Go to LOCAL using VISA Descriptor")
_viGTL("GPIB::1::0") ; Go to local (exit remote control mode)
MsgBox(0,"Step 4","Open the instrument connection with _viOpen")
Dim $h_instr = _viOpen(3)
MsgBox(0,"Instrument Handle obtained", "$h_instr = " & $h_instr) ; Show the Session Handle
; Query the instrument
MsgBox(0,"Step 5","Query the instrument using the VISA instrument handle")
$s_answer = _viExecCommand($h_instr,"*IDN?") ; $h_instr is NOT A STRING now!
MsgBox(0,"GPIB QUERY result",$s_answer) ; Show the answer
; Query again. There is no need to OPEN the link again
MsgBox(0,"Step 6","Query again. There is no need to OPEN the link again")
$s_answer = _viExecCommand($h_instr,"*IDN?")
MsgBox(0,"GPIB QUERY result",$s_answer) ; Show the answer
MsgBox(0,"Step 7","Go to LOCAL using VISA instrument handle")
_viGTL($h_instr); Go to local (this is optional)
MsgBox(0,"Step 8","Close the Instrument connection using _viClose")
_viClose($h_instr) ; Close the instrument connection